# Interface RangeDimension

All Known Subinterfaces:
  `Band`

All Known Implementing Classes:
  `DefaultBand, DefaultRangeDimension, DefaultSampleDimension`

@UML(identifier="MD_RangeDimension", specification=ISO_19115) public interface RangeDimension
Information on the range of each dimension of a cell measurement value.

Since:
  2.0

- ## Method Summary

  Modifier and Type
  Method
  Description
  `InternationalString`
  `getDescriptor()`
  Description of the range of a cell measurement value.
  `MemberName`
  `getSequenceIdentifier()`
  Number that uniquely identifies instances of bands of wavelengths on which a sensor operates.

- ## Method Details

  - ### getSequenceIdentifier

    @UML(identifier="sequenceIdentifier", obligation=OPTIONAL, specification=ISO_19115) MemberName getSequenceIdentifier()
    Number that uniquely identifies instances of bands of wavelengths on which a sensor operates.
    Returns:
      Identifier of bands on which a sensor operates, or `null`.

  - ### getDescriptor

    @UML(identifier="descriptor", obligation=OPTIONAL, specification=ISO_19115) InternationalString getDescriptor()
    Description of the range of a cell measurement value.
    Returns:
      Description of the range of a cell measurement value, or `null`.