# Uses of Package
org.opengis.referencing.cs

Packages that use org.opengis.referencing.cs
Package
Description
org.apache.sis.coverage.grid
A coverage backed by a regular grid.
org.apache.sis.io.wkt
Well Known Text (WKT) parsing and formatting.
org.apache.sis.referencing.crs
Coordinate Reference System (CRS) definitions as coordinate systems related to the earth through datum.
org.apache.sis.referencing.cs
Coordinate System (CS) definitions as the set of coordinate system axes that spans the coordinate space.
org.apache.sis.referencing.factory
Creates Coordinate Reference System (CRS) objects from given properties or authority codes.
org.apache.sis.referencing.factory.sql
Factories for geodetic objects defined in a SQL database, typically the EPSG dataset.
org.apache.sis.referencing.operation
Relationship between any two Coordinate Reference Systems (CRS).
org.apache.sis.referencing.operation.matrix
Matrix implementations for spatiotemporal referencing.
org.apache.sis.referencing.operation.transform
Conversions or transformations of multi-dimensional coordinate tuples.
org.apache.sis.util
Simple data objects and miscellaneous utilities.
org.opengis.referencing.crs
Coordinate reference systems (coordinate systems with a datum).
org.opengis.referencing.cs
Coordinate systems and their axis.
org.opengis.referencing.operation
Coordinate operations (relationship between any two coordinate reference systems).

- Classes in org.opengis.referencing.cs used by org.apache.sis.coverage.grid
  Class
  Description
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
  CoordinateSystemAxis
  Definition of a coordinate system axis.
- Classes in org.opengis.referencing.cs used by org.apache.sis.io.wkt
  Class
  Description
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.crs
  Class
  Description
  CartesianCS
  A 1-, 2-, or 3-dimensional coordinate system.
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
  EllipsoidalCS
  A two- or three-dimensional coordinate system in which position is specified by geodetic latitude, geodetic longitude, and (in the three-dimensional case) ellipsoidal height.
  SphericalCS
  A three-dimensional coordinate system with one distance measured from the origin and two angular coordinates.
  TimeCS
  A one-dimensional coordinate system containing a single time axis, used to describe the temporal position of a point in the specified time units from a specified time origin.
  VerticalCS
  A one-dimensional coordinate system used to record the heights (or depths) of points.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.cs
  Class
  Description
  AffineCS
  A two- or three-dimensional coordinate system with straight axes that are not necessarily orthogonal.
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
  CartesianCS
  A 1-, 2-, or 3-dimensional coordinate system.
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
  CoordinateSystemAxis
  Definition of a coordinate system axis.
  CylindricalCS
  A three-dimensional coordinate system consisting of a polar coordinate system extended by a straight coordinate axis perpendicular to the plane spanned by the polar coordinate system.
  EllipsoidalCS
  A two- or three-dimensional coordinate system in which position is specified by geodetic latitude, geodetic longitude, and (in the three-dimensional case) ellipsoidal height.
  LinearCS
  A one-dimensional coordinate system that consists of the points that lie on the single axis described.
  PolarCS
  A two-dimensional coordinate system in which position is specified by the distance from the origin and the angle between the line from the origin to a point and a reference direction.
  RangeMeaning
  Meaning of the axis value range specified through minimum value and maximum value.
  SphericalCS
  A three-dimensional coordinate system with one distance measured from the origin and two angular coordinates.
  TimeCS
  A one-dimensional coordinate system containing a single time axis, used to describe the temporal position of a point in the specified time units from a specified time origin.
  VerticalCS
  A one-dimensional coordinate system used to record the heights (or depths) of points.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.factory
  Class
  Description
  AffineCS
  A two- or three-dimensional coordinate system with straight axes that are not necessarily orthogonal.
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
  CartesianCS
  A 1-, 2-, or 3-dimensional coordinate system.
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
  CoordinateSystemAxis
  Definition of a coordinate system axis.
  CSAuthorityFactory
  Creates coordinate systems using authority codes.
  CSFactory
  Builds up complex coordinate systems from simpler objects or values.
  CylindricalCS
  A three-dimensional coordinate system consisting of a polar coordinate system extended by a straight coordinate axis perpendicular to the plane spanned by the polar coordinate system.
  EllipsoidalCS
  A two- or three-dimensional coordinate system in which position is specified by geodetic latitude, geodetic longitude, and (in the three-dimensional case) ellipsoidal height.
  LinearCS
  A one-dimensional coordinate system that consists of the points that lie on the single axis described.
  PolarCS
  A two-dimensional coordinate system in which position is specified by the distance from the origin and the angle between the line from the origin to a point and a reference direction.
  SphericalCS
  A three-dimensional coordinate system with one distance measured from the origin and two angular coordinates.
  TimeCS
  A one-dimensional coordinate system containing a single time axis, used to describe the temporal position of a point in the specified time units from a specified time origin.
  UserDefinedCS
  A two- or three-dimensional coordinate system that consists of any combination of coordinate axes not covered by any other Coordinate System type.
  VerticalCS
  A one-dimensional coordinate system used to record the heights (or depths) of points.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.factory.sql
  Class
  Description
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
  CoordinateSystemAxis
  Definition of a coordinate system axis.
  CSAuthorityFactory
  Creates coordinate systems using authority codes.
  CSFactory
  Builds up complex coordinate systems from simpler objects or values.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.operation
  Class
  Description
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.operation.matrix
  Class
  Description
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
- Classes in org.opengis.referencing.cs used by org.apache.sis.referencing.operation.transform
  Class
  Description
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
- Classes in org.opengis.referencing.cs used by org.apache.sis.util
  Class
  Description
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
- Classes in org.opengis.referencing.cs used by org.opengis.referencing.crs
  Class
  Description
  AffineCS
  A two- or three-dimensional coordinate system with straight axes that are not necessarily orthogonal.
  CartesianCS
  A 1-, 2-, or 3-dimensional coordinate system.
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
  EllipsoidalCS
  A two- or three-dimensional coordinate system in which position is specified by geodetic latitude, geodetic longitude, and (in the three-dimensional case) ellipsoidal height.
  SphericalCS
  A three-dimensional coordinate system with one distance measured from the origin and two angular coordinates.
  TimeCS
  A one-dimensional coordinate system containing a single time axis, used to describe the temporal position of a point in the specified time units from a specified time origin.
  VerticalCS
  A one-dimensional coordinate system used to record the heights (or depths) of points.
- Classes in org.opengis.referencing.cs used by org.opengis.referencing.cs
  Class
  Description
  AffineCS
  A two- or three-dimensional coordinate system with straight axes that are not necessarily orthogonal.
  AxisDirection
  The direction of positive increments in the coordinate value for a coordinate system axis.
  CartesianCS
  A 1-, 2-, or 3-dimensional coordinate system.
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.
  CoordinateSystemAxis
  Definition of a coordinate system axis.
  CylindricalCS
  A three-dimensional coordinate system consisting of a polar coordinate system extended by a straight coordinate axis perpendicular to the plane spanned by the polar coordinate system.
  EllipsoidalCS
  A two- or three-dimensional coordinate system in which position is specified by geodetic latitude, geodetic longitude, and (in the three-dimensional case) ellipsoidal height.
  LinearCS
  A one-dimensional coordinate system that consists of the points that lie on the single axis described.
  PolarCS
  A two-dimensional coordinate system in which position is specified by the distance from the origin and the angle between the line from the origin to a point and a reference direction.
  RangeMeaning
  Meaning of the axis value range specified through minimum value and maximum value.
  SphericalCS
  A three-dimensional coordinate system with one distance measured from the origin and two angular coordinates.
  TimeCS
  A one-dimensional coordinate system containing a single time axis, used to describe the temporal position of a point in the specified time units from a specified time origin.
  UserDefinedCS
  A two- or three-dimensional coordinate system that consists of any combination of coordinate axes not covered by any other Coordinate System type.
  VerticalCS
  A one-dimensional coordinate system used to record the heights (or depths) of points.
- Classes in org.opengis.referencing.cs used by org.opengis.referencing.operation
  Class
  Description
  CoordinateSystem
  The set of coordinate system axes that spans a given coordinate space.