# Uses of Package
org.opengis.referencing.crs

Packages that use org.opengis.referencing.crs
Package
Description
org.apache.sis.coordinate
Tuple of coordinate values.
org.apache.sis.coverage
Functions that associates positions within a bounded space (its domain) to values (its range).
org.apache.sis.coverage.grid
A coverage backed by a regular grid.
org.apache.sis.feature
Defines the structure and content of views of real-world phenomenon.
org.apache.sis.feature.builder
Helper classes for creating `FeatureType` instances.
org.apache.sis.filter
Filters features according their properties.
org.apache.sis.geometry
Basic geometric objects (envelopes and direct positions).
org.apache.sis.gui.referencing
Widgets about coordinate reference systems.
org.apache.sis.index.tree
A simple k-dimensional point tree implementation.
org.apache.sis.metadata.iso.extent
Information about spatial, vertical, and temporal extent.
org.apache.sis.portrayal
Symbology and map representations, together with a rendering engine for display.
org.apache.sis.referencing
Base classes for reference systems used for general positioning.
org.apache.sis.referencing.crs
Coordinate Reference System (CRS) definitions as coordinate systems related to the earth through datum.
org.apache.sis.referencing.datum
Relationship of a `CoordinateSystem` (an abstract mathematical entity) to the earth or other system.
org.apache.sis.referencing.factory
Creates Coordinate Reference System (CRS) objects from given properties or authority codes.
org.apache.sis.referencing.factory.sql
Factories for geodetic objects defined in a SQL database, typically the EPSG dataset.
org.apache.sis.referencing.gazetteer
Mapping between geographic identifiers (addresses, grid indexes…) and locations (descriptions, coordinates…).
org.apache.sis.referencing.operation
Relationship between any two Coordinate Reference Systems (CRS).
org.apache.sis.referencing.operation.transform
Conversions or transformations of multi-dimensional coordinate tuples.
org.apache.sis.setup
Provides information and some controls about Apache SIS configuration.
org.apache.sis.storage.aggregate
Resources which are aggregations or concatenations of other resources.
org.apache.sis.storage.sql
Data store capable to read and write features using a JDBC connection to a database.
org.apache.sis.storage.tiling
Base types for retrieving and saving tiles in resources.
org.apache.sis.util
Simple data objects and miscellaneous utilities.
org.opengis.geometry
org.opengis.metadata.extent
Extent information.
org.opengis.referencing.crs
Coordinate reference systems (coordinate systems with a datum).
org.opengis.referencing.operation
Coordinate operations (relationship between any two coordinate reference systems).

- Classes in org.opengis.referencing.crs used by org.apache.sis.coordinate
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.coverage
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.coverage.grid
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  DerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system but is not a projected coordinate reference system.
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
- Classes in org.opengis.referencing.crs used by org.apache.sis.feature
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.feature.builder
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.filter
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.geometry
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.gui.referencing
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  CRSAuthorityFactory
  Creates coordinate reference systems using authority codes.
  GeographicCRS
  A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
  ProjectedCRS
  A 2D coordinate reference system used to approximate the shape of the earth on a planar surface.
- Classes in org.opengis.referencing.crs used by org.apache.sis.index.tree
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.metadata.iso.extent
  Class
  Description
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.apache.sis.portrayal
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  EngineeringCRS
  A contextually local coordinate reference system.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  CRSAuthorityFactory
  Creates coordinate reference systems using authority codes.
  EngineeringCRS
  A contextually local coordinate reference system.
  GeocentricCRS
  A 3D coordinate reference system with the origin at the approximate centre of mass of the earth.
  GeodeticCRS
  A coordinate reference system associated with a geodetic datum.
  GeographicCRS
  A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
  ProjectedCRS
  A 2D coordinate reference system used to approximate the shape of the earth on a planar surface.
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
  TemporalCRS
  A 1D coordinate reference system used for the recording of time.
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.crs
  Class
  Description
  CompoundCRS
  A coordinate reference system describing the position of points through two or more independent coordinate reference systems.
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  DerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system but is not a projected coordinate reference system.
  EngineeringCRS
  A contextually local coordinate reference system.
  GeneralDerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system (not by a datum).
  GeocentricCRS
  A 3D coordinate reference system with the origin at the approximate centre of mass of the earth.
  GeodeticCRS
  A coordinate reference system associated with a geodetic datum.
  GeographicCRS
  A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
  ProjectedCRS
  A 2D coordinate reference system used to approximate the shape of the earth on a planar surface.
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
  TemporalCRS
  A 1D coordinate reference system used for the recording of time.
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.datum
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  EngineeringCRS
  A contextually local coordinate reference system.
  GeodeticCRS
  A coordinate reference system associated with a geodetic datum.
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
  TemporalCRS
  A 1D coordinate reference system used for the recording of time.
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.factory
  Class
  Description
  CompoundCRS
  A coordinate reference system describing the position of points through two or more independent coordinate reference systems.
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  CRSAuthorityFactory
  Creates coordinate reference systems using authority codes.
  CRSFactory
  Builds up complex coordinate reference systems from simpler objects or values.
  DerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system but is not a projected coordinate reference system.
  EngineeringCRS
  A contextually local coordinate reference system.
  GeocentricCRS
  A 3D coordinate reference system with the origin at the approximate centre of mass of the earth.
  GeodeticCRS
  A coordinate reference system associated with a geodetic datum.
  GeographicCRS
  A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
  ImageCRS
  An engineering coordinate reference system applied to locations in images.
  ProjectedCRS
  A 2D coordinate reference system used to approximate the shape of the earth on a planar surface.
  TemporalCRS
  A 1D coordinate reference system used for the recording of time.
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.factory.sql
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  CRSAuthorityFactory
  Creates coordinate reference systems using authority codes.
  CRSFactory
  Builds up complex coordinate reference systems from simpler objects or values.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.gazetteer
  Class
  Description
  GeographicCRS
  A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.operation
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  GeneralDerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system (not by a datum).
  GeodeticCRS
  A coordinate reference system associated with a geodetic datum.
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
  TemporalCRS
  A 1D coordinate reference system used for the recording of time.
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.apache.sis.referencing.operation.transform
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.setup
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.storage.aggregate
  Class
  Description
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
- Classes in org.opengis.referencing.crs used by org.apache.sis.storage.sql
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.storage.tiling
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.apache.sis.util
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.opengis.geometry
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
- Classes in org.opengis.referencing.crs used by org.opengis.metadata.extent
  Class
  Description
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.opengis.referencing.crs
  Class
  Description
  CompoundCRS
  A coordinate reference system describing the position of points through two or more independent coordinate reference systems.
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.
  DerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system but is not a projected coordinate reference system.
  EngineeringCRS
  A contextually local coordinate reference system.
  GeneralDerivedCRS
  A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system (not by a datum).
  GeocentricCRS
  A 3D coordinate reference system with the origin at the approximate centre of mass of the earth.
  GeodeticCRS
  A coordinate reference system associated with a geodetic datum.
  GeographicCRS
  A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
  ImageCRS
  An engineering coordinate reference system applied to locations in images.
  ProjectedCRS
  A 2D coordinate reference system used to approximate the shape of the earth on a planar surface.
  SingleCRS
  Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
  TemporalCRS
  A 1D coordinate reference system used for the recording of time.
  VerticalCRS
  A 1D coordinate reference system used for recording heights or depths.
- Classes in org.opengis.referencing.crs used by org.opengis.referencing.operation
  Class
  Description
  CoordinateReferenceSystem
  Abstract coordinate reference system, usually defined by a coordinate system and a datum.